GDB Internals

Node:Algorithms, Next:User Interface, Previous:Overall Structure, Up:Top

## Algorithms

GDB uses a number of debugging-specific algorithms. They are often not very complicated, but get lost in the thicket of special cases and real-world issues. This chapter describes the basic algorithms and mentions some of the specific target definitions that they use.

### Frames

A frame is a construct that GDB uses to keep track of calling and called functions.

`FRAME_FP` in the machine description has no meaning to the machine-independent part of GDB, except that it is used when setting up a new frame from scratch, as follows:

               create_new_frame (read_register (FP_REGNUM), read_pc ()));

Other than that, all the meaning imparted to `FP_REGNUM` is imparted by the machine-dependent code. So, `FP_REGNUM` can have any value that is convenient for the code that creates new frames. (`create_new_frame` calls `INIT_EXTRA_FRAME_INFO` if it is defined; that is where you should use the `FP_REGNUM` value, if your frames are nonstandard.)

Given a GDB frame, define `FRAME_CHAIN` to determine the address of the calling function's frame. This will be used to create a new GDB frame struct, and then `INIT_EXTRA_FRAME_INFO` and `INIT_FRAME_PC` will be called for the new frame.

### Breakpoint Handling

In general, a breakpoint is a user-designated location in the program where the user wants to regain control if program execution ever reaches that location.

There are two main ways to implement breakpoints; either as "hardware" breakpoints or as "software" breakpoints.

Hardware breakpoints are sometimes available as a builtin debugging features with some chips. Typically these work by having dedicated register into which the breakpoint address may be stored. If the PC (shorthand for program counter) ever matches a value in a breakpoint registers, the CPU raises an exception and reports it to GDB.

Another possibility is when an emulator is in use; many emulators include circuitry that watches the address lines coming out from the processor, and force it to stop if the address matches a breakpoint's address.

A third possibility is that the target already has the ability to do breakpoints somehow; for instance, a ROM monitor may do its own software breakpoints. So although these are not literally "hardware breakpoints", from GDB's point of view they work the same; GDB need not do nothing more than set the breakpoint and wait for something to happen.

Since they depend on hardware resources, hardware breakpoints may be limited in number; when the user asks for more, GDB will start trying to set software breakpoints. (On some architectures, notably the 32-bit x86 platforms, GDB cannot alsways know whether there's enough hardware resources to insert all the hardware breakpoints and watchpoints. On those platforms, GDB prints an error message only when the program being debugged is continued.)

Software breakpoints require GDB to do somewhat more work. The basic theory is that GDB will replace a program instruction with a trap, illegal divide, or some other instruction that will cause an exception, and then when it's encountered, GDB will take the exception and stop the program. When the user says to continue, GDB will restore the original instruction, single-step, re-insert the trap, and continue on.

Since it literally overwrites the program being tested, the program area must be writable, so this technique won't work on programs in ROM. It can also distort the behavior of programs that examine themselves, although such a situation would be highly unusual.

Also, the software breakpoint instruction should be the smallest size of instruction, so it doesn't overwrite an instruction that might be a jump target, and cause disaster when the program jumps into the middle of the breakpoint instruction. (Strictly speaking, the breakpoint must be no larger than the smallest interval between instructions that may be jump targets; perhaps there is an architecture where only even-numbered instructions may jumped to.) Note that it's possible for an instruction set not to have any instructions usable for a software breakpoint, although in practice only the ARC has failed to define such an instruction.

The basic definition of the software breakpoint is the macro `BREAKPOINT`.

Basic breakpoint object handling is in `breakpoint.c`. However, much of the interesting breakpoint action is in `infrun.c`.

### Single Stepping

### Signal Handling

### Thread Handling

### Inferior Function Calls

### Longjmp Support

GDB has support for figuring out that the target is doing a `longjmp` and for stopping at the target of the jump, if we are stepping. This is done with a few specialized internal breakpoints, which are visible in the output of the `maint info breakpoint` command.

To make this work, you need to define a macro called `GET_LONGJMP_TARGET`, which will examine the `jmp_buf` structure and extract the longjmp target address. Since `jmp_buf` is target specific, you will need to define it in the appropriate `tm-`target`.h` file. Look in `tm-sun4os4.h` and `sparc-tdep.c` for examples of how to do this.

### Watchpoints

Watchpoints are a special kind of breakpoints (see breakpoints) which break when data is accessed rather than when some instruction is executed. When you have data which changes without your knowing what code does that, watchpoints are the silver bullet to hunt down and kill such bugs.

Watchpoints can be either hardware-assisted or not; the latter type is known as "software watchpoints." GDB always uses hardware-assisted watchpoints if they are available, and falls back on software watchpoints otherwise. Typical situations where GDB will use software watchpoints are:

- The watched memory region is too large for the underlying hardware watchpoint support. For example, each x86 debug register can watch up to 4 bytes of memory, so trying to watch data structures whose size is more than 16 bytes will cause GDB to use software watchpoints.
- The value of the expression to be watched depends on data held in registers (as opposed to memory).
- Too many different watchpoints requested. (On some architectures, this situation is impossible to detect until the debugged program is resumed.) Note that x86 debug registers are used both for hardware breakpoints and for watchpoints, so setting too many hardware breakpoints might cause watchpoint insertion to fail.
- No hardware-assisted watchpoints provided by the target implementation.

Software watchpoints are very slow, since GDB needs to single-step the program being debugged and test the value of the watched expression(s) after each instruction. The rest of this section is mostly irrelevant for software watchpoints. GDB uses several macros and primitives to support hardware watchpoints:

`TARGET_HAS_HARDWARE_WATCHPOINTS`
  If defined, the target supports hardware watchpoints.
`TARGET_CAN_USE_HARDWARE_WATCHPOINT (`type`,` count`,` other`)`
  Return the number of hardware watchpoints of type type that are possible to be set. The value is positive if count watchpoints of this type can be set, zero if setting watchpoints of this type is not supported, and negative if count is more than the maximum number of watchpoints of type type that can be set. other is non-zero if other types of watchpoints are currently enabled (there are architectures which cannot set watchpoints of different types at the same time).
`TARGET_REGION_OK_FOR_HW_WATCHPOINT (`addr`,` len`)`
  Return non-zero if hardware watchpoints can be used to watch a region whose address is addr and whose length in bytes is len.
`TARGET_REGION_SIZE_OK_FOR_HW_WATCHPOINT (`size`)`
  Return non-zero if hardware watchpoints can be used to watch a region whose size is size. GDB only uses this macro as a fall-back, in case `TARGET_REGION_OK_FOR_HW_WATCHPOINT` is not defined.
`TARGET_DISABLE_HW_WATCHPOINTS (`pid`)`
  Disables watchpoints in the process identified by pid. This is used, e.g., on HP-UX which provides operations to disable and enable the page-level memory protection that implements hardware watchpoints on that platform.
`TARGET_ENABLE_HW_WATCHPOINTS (`pid`)`
  Enables watchpoints in the process identified by pid. This is used, e.g., on HP-UX which provides operations to disable and enable the page-level memory protection that implements hardware watchpoints on that platform.
`target_insert_watchpoint (`addr`,` len`,` type`)`
`target_remove_watchpoint (`addr`,` len`,` type`)`
  Insert or remove a hardware watchpoint starting at addr, for len bytes. type is the watchpoint type, one of the possible values of the enumerated data type `target_hw_bp_type`, defined by `breakpoint.h` as follows:

                 enum target_hw_bp_type
                   {
                     hw_write   = 0, /* Common (write) HW watchpoint */
                     hw_read    = 1, /* Read    HW watchpoint */
                     hw_access  = 2, /* Access (read or write) HW watchpoint */
                     hw_execute = 3  /* Execute HW breakpoint */
                   };

  These two macros should return 0 for success, non-zero for failure.

`target_remove_hw_breakpoint (`addr`,` shadow`)`
`target_insert_hw_breakpoint (`addr`,` shadow`)`
  Insert or remove a hardware-assisted breakpoint at address addr. Returns zero for success, non-zero for failure. shadow is the real contents of the byte where the breakpoint has been inserted; it is generally not valid when hardware breakpoints are used, but since no other code touches these values, the implementations of the above two macros can use them for their internal purposes.
`target_stopped_data_address ()`
  If the inferior has some watchpoint that triggered, return the address associated with that watchpoint. Otherwise, return zero.
`DECR_PC_AFTER_HW_BREAK`
  If defined, GDB decrements the program counter by the value of `DECR_PC_AFTER_HW_BREAK` after a hardware break-point. This overrides the value of `DECR_PC_AFTER_BREAK` when a breakpoint that breaks is a hardware-assisted breakpoint.
`HAVE_STEPPABLE_WATCHPOINT`
  If defined to a non-zero value, it is not necessary to disable a watchpoint to step over it.
`HAVE_NONSTEPPABLE_WATCHPOINT`
  If defined to a non-zero value, GDB should disable a watchpoint to step the inferior over it.
`HAVE_CONTINUABLE_WATCHPOINT`
  If defined to a non-zero value, it is possible to continue the inferior after a watchpoint has been hit.
`CANNOT_STEP_HW_WATCHPOINTS`
  If this is defined to a non-zero value, GDB will remove all watchpoints before stepping the inferior.
`STOPPED_BY_WATCHPOINT (`wait_status`)`
  Return non-zero if stopped by a watchpoint. wait_status is of the type `struct target_waitstatus`, defined by `target.h`.

#### x86 Watchpoints

The 32-bit Intel x86 (a.k.a. ia32) processors feature special debug registers designed to facilitate debugging. GDB provides a generic library of functions that x86-based ports can use to implement support for watchpoints and hardware-assisted breakpoints. This subsection documents the x86 watchpoint facilities in GDB.

To use the generic x86 watchpoint support, a port should do the following:

- Define the macro `I386_USE_GENERIC_WATCHPOINTS` somewhere in the target-dependent headers.
- Include the `config/i386/nm-i386.h` header file after defining `I386_USE_GENERIC_WATCHPOINTS`.
- Add `i386-nat.o` to the value of the Make variable `NATDEPFILES` (see NATDEPFILES) or `TDEPFILES` (see TDEPFILES).
- Provide implementations for the `I386_DR_LOW_*` macros described below. Typically, each macro should call a target-specific function which does the real work.

The x86 watchpoint support works by maintaining mirror images of the debug registers. Values are copied between the mirror images and the real debug registers via a set of macros which each target needs to provide:

`I386_DR_LOW_SET_CONTROL (`val`)`
  Set the Debug Control (DR7) register to the value val.
`I386_DR_LOW_SET_ADDR (`idx`,` addr`)`
  Put the address addr into the debug register number idx.
`I386_DR_LOW_RESET_ADDR (`idx`)`
  Reset (i.e. zero out) the address stored in the debug register number idx.
`I386_DR_LOW_GET_STATUS`
  Return the value of the Debug Status (DR6) register. This value is used immediately after it is returned by `I386_DR_LOW_GET_STATUS`, so as to support per-thread status register values.

For each one of the 4 debug registers (whose indices are from 0 to 3) that store addresses, a reference count is maintained by GDB, to allow sharing of debug registers by several watchpoints. This allows users to define several watchpoints that watch the same expression, but with different conditions and/or commands, without wasting debug registers which are in short supply. GDB maintains the reference counts internally, targets don't have to do anything to use this feature.

The x86 debug registers can each watch a region that is 1, 2, or 4 bytes long. The ia32 architecture requires that each watched region be appropriately aligned: 2-byte region on 2-byte boundary, 4-byte region on 4-byte boundary. However, the x86 watchpoint support in GDB can watch unaligned regions and regions larger than 4 bytes (up to 16 bytes) by allocating several debug registers to watch a single region. This allocation of several registers per a watched region is also done automatically without target code intervention.

The generic x86 watchpoint support provides the following API for the GDB's application code:

`i386_region_ok_for_watchpoint (`addr`,` len`)`
  The macro `TARGET_REGION_OK_FOR_HW_WATCHPOINT` is set to call this function. It counts the number of debug registers required to watch a given region, and returns a non-zero value if that number is less than 4, the number of debug registers available to x86 processors.
`i386_stopped_data_address (void)`
  The macros `STOPPED_BY_WATCHPOINT` and `target_stopped_data_address` are set to call this function. The argument passed to `STOPPED_BY_WATCHPOINT` is ignored. This function examines the breakpoint condition bits in the DR6 Debug Status register, as returned by the `I386_DR_LOW_GET_STATUS` macro, and returns the address associated with the first bit that is set in DR6.
`i386_insert_watchpoint (`addr`,` len`,` type`)`
`i386_remove_watchpoint (`addr`,` len`,` type`)`
  Insert or remove a watchpoint. The macros `target_insert_watchpoint` and `target_remove_watchpoint` are set to call these functions. `i386_insert_watchpoint` first looks for a debug register which is already set to watch the same region for the same access types; if found, it just increments the reference count of that debug register, thus implementing debug register sharing between watchpoints. If no such register is found, the function looks for a vacant debug register, sets its mirrorred value to addr, sets the mirrorred value of DR7 Debug Control register as appropriate for the len and type parameters, and then passes the new values of the debug register and DR7 to the inferior by calling `I386_DR_LOW_SET_ADDR` and `I386_DR_LOW_SET_CONTROL`. If more than one debug register is required to cover the given region, the above process is repeated for each debug register.

  `i386_remove_watchpoint` does the opposite: it resets the address in the mirrorred value of the debug register and its read/write and length bits in the mirrorred value of DR7, then passes these new values to the inferior via `I386_DR_LOW_RESET_ADDR` and `I386_DR_LOW_SET_CONTROL`. If a register is shared by several watchpoints, each time a `i386_remove_watchpoint` is called, it decrements the reference count, and only calls `I386_DR_LOW_RESET_ADDR` and `I386_DR_LOW_SET_CONTROL` when the count goes to zero.

`i386_insert_hw_breakpoint (`addr`,` shadow``
`i386_remove_hw_breakpoint (`addr`,` shadow`)`
  These functions insert and remove hardware-assisted breakpoints. The macros `target_insert_hw_breakpoint` and `target_remove_hw_breakpoint` are set to call these functions. These functions work like `i386_insert_watchpoint` and `i386_remove_watchpoint`, respectively, except that they set up the debug registers to watch instruction execution, and each hardware-assisted breakpoint always requires exactly one debug register.
`i386_stopped_by_hwbp (void)`
  This function returns non-zero if the inferior has some watchpoint or hardware breakpoint that triggered. It works like `i386_stopped_data_address`, except that it doesn't return the address whose watchpoint triggered.
`i386_cleanup_dregs (void)`
  This function clears all the reference counts, addresses, and control bits in the mirror images of the debug registers. It doesn't affect the actual debug registers in the inferior process.

Notes:

1. x86 processors support setting watchpoints on I/O reads or writes. However, since no target supports this (as of March 2001), and since `enum target_hw_bp_type` doesn't even have an enumeration for I/O watchpoints, this feature is not yet available to GDB running on x86.
2. x86 processors can enable watchpoints locally, for the current task only, or globally, for all the tasks. For each debug register, there's a bit in the DR7 Debug Control register that determines whether the associated address is watched locally or globally. The current implementation of x86 watchpoint support in GDB always sets watchpoints to be locally enabled, since global watchpoints might interfere with the underlying OS and are probably unavailable in many platforms.