Debugging with GDB

Node:i960, Next:M32R/D, Previous:H8/500, Up:Embedded Processors

#### Intel i960

`target mon960` dev``
  MON960 monitor for Intel i960.
`target nindy` devicename``
  An Intel 960 board controlled by a Nindy Monitor. devicename is the name of the serial device to use for the connection, e.g. `/dev/ttya`.

Nindy is a ROM Monitor program for Intel 960 target systems. When GDB is configured to control a remote Intel 960 using Nindy, you can tell GDB how to connect to the 960 in several ways:

- Through command line options specifying serial port, version of the Nindy protocol, and communications speed;
- By responding to a prompt on startup;
- By using the `target` command at any point during your GDB session. See Commands for managing targets.

With the Nindy interface to an Intel 960 board, `load` downloads filename to the 960 as well as adding its symbols in GDB.