Debugging with GDB

Node:Nindy Startup, Next:Nindy Options, Up:i960

##### Startup with Nindy

If you simply start `gdb` without using any command-line options, you are prompted for what serial port to use, before you reach the ordinary GDB prompt:

         Attach /dev/ttyNN -- specify NN, or "quit" to quit:

Respond to the prompt with whatever suffix (after `/dev/tty`) identifies the serial port you want to use. You can, if you choose, simply start up with no Nindy connection by responding to the prompt with an empty line. If you do this and later wish to attach to Nindy, use `target` (see Commands for managing targets).