Debugging with GDB

Node:M68K, Next:M88K, Previous:M32R/D, Up:Embedded Processors

#### M68k

The Motorola m68k configuration includes ColdFire support, and target command for the following ROM monitors.

`target abug` dev``
  ABug ROM monitor for M68K.
`target cpu32bug` dev``
  CPU32BUG monitor, running on a CPU32 (M68K) board.
`target dbug` dev``
  dBUG ROM monitor for Motorola ColdFire.
`target est` dev``
  EST-300 ICE monitor, running on a CPU32 (M68K) board.
`target rom68k` dev``
  ROM 68K monitor, running on an M68K IDP board.

If GDB is configured with `m68*-ericsson-*`, it will instead have only a single special target command:

`target es1800` dev``
  ES-1800 emulator for M68K.

[context?]

`target rombug` dev``
  ROMBUG ROM monitor for OS/9000.