Debugging with GDB

Node:Hitachi ICE, Next:Hitachi Special, Previous:Hitachi Boards, Up:H8/300

##### Using the E7000 in-circuit emulator

You can use the E7000 in-circuit emulator to develop code for either the Hitachi SH or the H8/300H. Use one of these forms of the `target e7000` command to connect GDB to your E7000:

`target e7000` port`` speed``
  Use this form if your E7000 is connected to a serial port. The port argument identifies what serial port to use (for example, `com2`). The third argument is the line speed in bits per second (for example, `9600`).
`target e7000` hostname``
  If your E7000 is installed as a host on a TCP/IP network, you can just specify its hostname; GDB uses `telnet` to connect.